(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 15)
    (no_connects 0)
    (area 69.774999 31.674999 264.235001 155.015001)
    (thickness 1.6)
    (drawings 4)
    (tracks 45)
    (zones 0)
    (modules 9)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.75)
    (trace_clearance 0.6)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 1.000000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(R1-Pad2)")
  (net 4 "Net-(BT1-Pad1)")
  (net 5 +36V)
  (net_class Default "This is the default net class."
    (clearance 0.6)
    (trace_width 0.75)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +36V)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (module Connect:Banana_Jack_2Pin (layer F.Cu) (tedit 0)
    (at 200.66 104.14)
    (descr "Dual banana socket, footprint - 2 x 6mm drills")
    (tags "banana socket")
    (fp_text reference BT1 (at 0 1.27) (layer F.SilkS))
    (fp_text value "Battery 2000mAh or more" (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at -14.986 0) (size 10.16 10.16) (drill 6.096) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole circle (at 14.986 0) (size 10.16 10.16) (drill 6.096) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Connect.3dshapes/Banana_Jack_2Pin.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 134.62 78.74)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.25 -2.5) (layer F.SilkS))
    (fp_text value "C 0.33uf" (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 +36V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 148.59 78.74 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value "C 3.3uf 50v" (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_TO-220_Vertical (layer F.Cu) (tedit 5538AE5F)
    (at 208.28 78.74 270)
    (descr "TO-220, Diode, Vertical,")
    (tags "TO-220, Diode, Vertical,")
    (fp_text reference D1 (at 2.54762 -3.92938 270) (layer F.SilkS))
    (fp_text value D (at 2.0701 2.7051 270) (layer F.Fab))
    (fp_text user A (at 6.858 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(BT1-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_TO-220_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:Banana_Jack_2Pin (layer F.Cu) (tedit 0)
    (at 86.36 86.36 90)
    (descr "Dual banana socket, footprint - 2 x 6mm drills")
    (tags "banana socket")
    (fp_text reference P1 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.27 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -14.986 0 90) (size 10.16 10.16) (drill 6.096) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 14.986 0 90) (size 10.16 10.16) (drill 6.096) (layers *.Cu *.Mask F.SilkS)
      (net 5 +36V))
    (model Connect.3dshapes/Banana_Jack_2Pin.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:Banana_Jack_2Pin (layer F.Cu) (tedit 57AB7895)
    (at 233.68 88.9 270)
    (descr "Dual banana socket, footprint - 2 x 6mm drills")
    (tags "banana socket")
    (fp_text reference P2 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.27 360) (layer F.Fab))
    (pad 1 thru_hole circle (at -14.986 0 270) (size 10.16 10.16) (drill 6.096) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 14.986 0 270) (size 10.16 10.16) (drill 6.096) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Connect.3dshapes/Banana_Jack_2Pin.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Cement_Vertical_LargePads_KOA-BGR-5N-7N (layer F.Cu) (tedit 0)
    (at 187.96 82.55 90)
    (descr "Resistor, Cement, Vertical, LargePads, 5W, 7W, Meggitt, KOA, BSR, BGR, BWR, 5N, 7N,")
    (tags "Resistor, Cement, Vertical, 5W, 7W, Meggitt, KOA, BSR, LargePads, BGR, BWR, 5N, 7N,")
    (fp_text reference R1 (at 0 -7.00024 90) (layer F.SilkS))
    (fp_text value 10 (at 0 8.49884 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -2.49936 0 90) (size 2.99974 1.99898) (drill 1.19888 (offset -0.50038 0)) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole oval (at 2.49936 0 270) (size 2.99974 1.99898) (drill 1.19888 (offset -0.50038 0)) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(R1-Pad2)"))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 137.16 71.12)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U1 (at 0 -4.318) (layer F.SilkS))
    (fp_text value LM7815CT (at 0 -4.318) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C2-Pad1)"))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 5 +36V))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 168.91 81.28 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U2 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value LM317T (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(R1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C2-Pad1)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(BT1-Pad1)"))
  )
  (gr_line (start 264.16 154.94) (end 264.16 31.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 69.85 31.75) (end 69.85 154.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 264.16 154.94) (end 69.85 154.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 69.85 31.75) (end 264.16 31.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 81.28) (xy 151.13 81.28) (xy 156.21 86.36) (xy 158.75 87.63) (xy 158.75 92.71)
        (xy 179.07 113.03) (xy 190.5 113.03) (xy 201.93 101.6) (xy 242.57 101.6) (xy 242.57 119.38)
        (xy 81.28 118.11) (xy 81.28 96.52) (xy 114.3 96.52) (xy 137.16 78.74) (xy 139.7 81.28)
      )
    )
  )
  (zone (net 5) (net_name +36V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.62 80.01) (xy 82.55 80.01) (xy 82.55 68.58) (xy 134.62 68.58) (xy 134.62 80.01)
      )
    )
  )
  (zone (net 3) (net_name "Net-(R1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 238.76 78.74) (xy 238.76 67.31) (xy 139.7 66.04) (xy 139.7 77.47) (xy 181.61 77.47)
        (xy 181.61 76.2) (xy 200.66 76.2) (xy 200.66 80.01) (xy 238.76 80.01) (xy 238.76 76.2)
      )
    )
  )
)
