(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 35)
    (no_connects 0)
    (area 132.004999 57.074999 251.535001 120.725001)
    (thickness 1.6)
    (drawings 14)
    (tracks 110)
    (zones 0)
    (modules 20)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.7)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 9.4 10.8)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 132.08 120.65)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(IC1-Pad1)")
  (net 6 "Net-(IC1-Pad7)")
  (net 7 "Net-(IC1-Pad10)")
  (net 8 "Net-(IC1-Pad11)")
  (net 9 "Net-(IC1-Pad12)")
  (net 10 "Net-(IC1-Pad14)")
  (net 11 "Net-(U1-Pad10)")
  (net 12 VDD)
  (net 13 "Net-(P1-Pad1)")
  (net 14 "Net-(P3-Pad1)")
  (net 15 "Net-(P5-Pad1)")
  (net 16 "Net-(C3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.7)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net VDD)
  )
  (module Connect:1pin (layer F.Cu) (tedit 0)
    (at 196.85 72.39)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P5 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P5-Pad1)"))
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 579EC423)
    (at 180.34 78.74 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value .1uf (at -2.54 0 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-10MM (layer F.Cu) (tedit 55BDE3C5)
    (at 237.49 76.2)
    (descr "LED 10mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 10mm 10MM 100mil 2.54mm")
    (fp_text reference D1 (at 1.27 -6.25) (layer F.SilkS))
    (fp_text value LED (at 1.5 6.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model LEDs.3dshapes/LED-10MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-10MM (layer F.Cu) (tedit 55BDE3C5)
    (at 237.49 100.33)
    (descr "LED 10mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 10mm 10MM 100mil 2.54mm")
    (fp_text reference D2 (at 1.27 -6.25) (layer F.SilkS))
    (fp_text value LED (at 1.5 6.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (model LEDs.3dshapes/LED-10MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:D3 (layer F.Cu) (tedit 579EC43F)
    (at 198.12 83.82 270)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D3 (at 0 0 270) (layer F.SilkS))
    (fp_text value "ZENER 5v IN4625" (at -1.27 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 VDD))
    (model Discret.3dshapes/D3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 579EC417)
    (at 170.18 78.74 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 4.05892 -3.50012 270) (layer F.SilkS))
    (fp_text value 470K (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(IC1-Pad11)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 579EC4B9)
    (at 191.77 80.01 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R5 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value "330 ohm 1/2 watt" (at -3.81 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 VDD))
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 0)
    (at 191.77 96.52 90)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 4011 (at 0 1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad7)"))
    (pad 2 smd rect (at -2.54 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad1)"))
    (pad 3 smd rect (at -1.27 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P1-Pad1)"))
    (pad 4 smd rect (at 0 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P3-Pad1)"))
    (pad 5 smd rect (at 1.27 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C3-Pad1)"))
    (pad 6 smd rect (at 2.54 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C3-Pad1)"))
    (pad 7 smd rect (at 3.81 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 3.81 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad1)"))
    (pad 9 smd rect (at 2.54 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad14)"))
    (pad 11 smd rect (at 0 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad12)"))
    (pad 12 smd rect (at -1.27 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.54 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad10)"))
    (pad 14 smd rect (at -3.81 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 VDD))
    (pad 10 smd rect (at 1.27 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad10)"))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 0)
    (at 204.47 106.68)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P1 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P1-Pad1)"))
  )
  (module Connect:1pin (layer F.Cu) (tedit 0)
    (at 204.47 90.17)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P2 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C3-Pad1)"))
  )
  (module Connect:1pin (layer F.Cu) (tedit 0)
    (at 204.47 97.79)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P3 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P3-Pad1)"))
  )
  (module TO_SOT_Packages_THT:TO-18_3Pin (layer F.Cu) (tedit 57A122C1)
    (at 233.68 88.9 90)
    (descr "TO-18, 3Pin,")
    (tags "TO-18, 3Pin,")
    (fp_text reference T1 (at 0.254 -4.826 90) (layer F.SilkS))
    (fp_text value "NPN, MPSA18 (cbe), BC337 (cbe), 2N4401 (ebc)" (at 0 -2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.27 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 -1.27 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C3-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-18_3Pin.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 240.03 88.9 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value "C .02uf" (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 579EC888)
    (at 204.47 78.74)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P4 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module SMD_Packages:SO-16-N (layer F.Cu) (tedit 579EC4EB)
    (at 176.53 95.25)
    (descr "Module CMS SOJ 16 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference IC1 (at 0.127 -1.27) (layer F.SilkS))
    (fp_text value 4060D (at -8.89 0) (layer F.Fab))
    (pad 16 smd rect (at -4.445 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad14)"))
    (pad 13 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad12)"))
    (pad 11 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad11)"))
    (pad 10 smd rect (at 3.175 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad10)"))
    (pad 9 smd rect (at 4.445 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 8 smd rect (at 4.445 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.175 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad7)"))
    (pad 6 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.175 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -4.445 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad1)"))
    (pad 15 smd rect (at -3.175 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SO-16-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:1pin placed (layer F.Cu) (tedit 579EC893)
    (at 204.47 72.39)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P6 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 12 VDD))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 579EC0B1)
    (at 227.33 92.71 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 4.05892 -3.50012 90) (layer F.SilkS))
    (fp_text value 330K (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 16 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 VDD))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 579EC410)
    (at 175.26 78.74 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 4.05892 -3.50012 270) (layer F.SilkS))
    (fp_text value 100K (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(IC1-Pad10)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 579EC4A6)
    (at 185.42 80.01 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at -3.81 0 270) (layer F.SilkS))
    (fp_text value 47K (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(IC1-Pad12)"))
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 204.47 85.09 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value "C .02uf" (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Supply +22v max to P5 \nor +5v max P6 (not to both)." (at 200.66 66.04) (layer F.Cu))
  (gr_text "Bridge outputs\nhigh/low (P2,P3)\nenable (low,P1)" (at 213.36 104.14 90) (layer F.Cu))
  (gr_text "Remote Sun sensor\nVDC+ and -, plus\nreturn signal; ie.\nthree wires." (at 233.68 62.23) (layer F.Cu))
  (gr_text "The 4060 component omitted\nthe power +15v to pin 16, and\nGND pin 8. So I added backside\nfill to remind me of the error." (at 173.99 109.22) (layer F.Cu))
  (gr_line (start 132.08 120.65) (end 251.46 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 251.46 57.15) (end 251.46 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 57.15) (end 251.46 57.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 120.65) (end 132.08 57.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.72 91.44) (xy 170.18 92.71) (xy 170.18 100.33) (xy 189.23 100.33) (xy 189.23 101.6)
        (xy 168.91 101.6) (xy 168.91 90.17) (xy 172.72 90.17) (xy 172.72 91.44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 181.61 97.79) (xy 184.15 97.79) (xy 185.42 90.17) (xy 195.58 90.17) (xy 196.85 86.36)
        (xy 199.39 86.36) (xy 199.39 88.9) (xy 199.39 91.44) (xy 186.69 91.44) (xy 185.42 99.06)
        (xy 180.34 99.06) (xy 180.34 97.79)
      )
    )
  )
)
